Clause 30 YANG review summary
Reviewed 1 module(s): 9 finding(s), 33 reference check(s), and 3 prose warning(s). These are review candidates and require human assessment.
Reference and attribute overview
Reference statuses: found: 33
Unreferenced attributes: 527; uncertain attributes: 0. An unreferenced attribute is not necessarily absent from a model.
Findings by module
/home/petejone/yang/git_802_3/yang_main/Modules/Approved/ieee802-ethernet-interface.yang
Disabled negotiation cannot report no-negotiation. The when condition hides this leaf when enable is false, although its no-negotiation enum describes a disabled function.
Line 221; ethernet/auto-negotiation/negotiation-status; Clause 30.6.1.1.4
Parallel detect failure has no explicit mapping. The referenced attribute distinguishes parallel detect failure; the leaf does not name that condition in an enum. Review the mapping to failed.
Line 221; ethernet/auto-negotiation/negotiation-status; Clause 30.6.1.1.4
PMD to MAU mapping needs review. The referenced MAU enumeration includes state and complete MAU distinctions. Confirm how these map to the imported PMD identities. RFC 9907 review context: rfc9907-4.11.1-1 https://www.rfc-editor.org/rfc/rfc9907.html#section-4.11.1 RFC 9907 review context: rfc9907-4.11.1-3 https://www.rfc-editor.org/rfc/rfc9907.html#section-4.11.1
Line 271; ethernet/pmd-type; Clause 30.5.1.1.2
Operational duplex is modeled as configuration. The description calls this operational state, but the leaf is writable by default. Clause 30 specifies both GET and SET behavior; clarify the configuration and state mapping. RFC 9907 review context: rfc9907-4.23.1-1 https://www.rfc-editor.org/rfc/rfc9907.html#section-4.23.1
Line 282; ethernet/duplex; Clause 30.3.1.1.32
Receive counter describes transmission. The node and referenced attribute identify received events, while the node description says transmitted.
Line 333; ethernet/flow-control/pause/statistics/in-frames-pause; Clause 30.3.4.3
Frame length has no explicit unknown value. The numeric leaf has no documented representation for the unknown value in the referenced enumeration.
Line 429; ethernet/max-frame-length; Clause 30.3.1.1.37
Extension status exposes only read access. The referenced attribute supports reading and setting; this leaf is config false. Confirm whether the restricted mapping is intentional.
Line 439; ethernet/mac-control-extension-control; Clause 30.3.8.3
Receive counter describes transmission. The node and referenced attribute identify received events, while the node description says transmitted.
Line 534; ethernet/ethernet-pause/statistics/in-frames-pause; Clause 30.3.4.3
Symbol-error summary suggests counting individual errors. The referenced attribute counts qualifying carrier events with one or more errors, at most once per valid event and subject to collision conditions.
Line 793; ethernet/statistics/phy/in-error-symbol; Clause 30.3.2.1.5
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Review limitations
Rule-based review only; it does not establish semantic conformance or cover every model mapping.
Unreferenced attributes have no explicit IEEE 802.3 section reference in the selected modules; implicit, inherited, name-only, and external mappings are not resolved. Unqualified references are uncertain; referenced duplicate section IDs are excluded from this inventory.
Package mapping guidance consists of review candidates, not mandatory or approved mappings. Derived YANG types are not resolved.
RFC 9907 candidate labels and uppercase terms are heuristic review aids, not applicability or conformance determinations; examples and context require review.
Prose checks detect repeated words or phrases and possible spelling problems, not full grammar; technical terms and extracted text can cause false positives.
The lightweight YANG statement reader does not validate syntax, resolve imports, expand groupings, or apply augments and deviations.
Checks depend on extracted text; verify findings against the authoritative standard and related procedures.
Package checksums establish consistency, not publisher authenticity.
See the accompanying Excel, HTML, and JSON reports for detailed reference checks, guidance, prose warnings, inventories, and environment information.
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